In the determination of both the Fourier cosine series and full Fourier series the values for a0, an, and bn are typically determined by an integral featuring a function f(x).However, given that there is no function given for the rocket data set, the integrals were evaluated as a series. The transition can be found below.

For the values from a to b, the integral of the function is equal to the summation of all f(x) values multiplied by a very small change in x. For the cosine series, it was only necessary to calculate a0 and an. The integrals for these values are given as

In series notation, these would be given by

In this case, L would vary over a 50s time frame from 850 to 900 seconds in the flight for the given data set. The full Fourier series would be given by

Substituting the values for a0, an, and bn, the Fourier series would be given by

Using a similar fashion, the cosine series would be given by

For the full Fourier series, the value of bn would have to be calculated slightly differently. As the sine expansion is not symmetric about the y axis, the value for bn would have to be calculated from -50s to 0s and from 0s to 50s and then added together. The values for the density would stay the same over both intervals.

This calculation can be completed in MATLAB through a pair of nested for loops, calculating the values of the coefficients over the range of x values from -50s to 50s and determining those values for each of the n number of terms (5, 7, and 10 in this case).